|  |  |
| --- | --- |
|  | NTS 2.0 Radiogram Handling Instructions |
|  |  |
|  | NOTE: If more than one HX prosign is used, they can be combined if no numbers are to be inserted, otherwise the HX should be repeated thus: NR 207 R HXCE W4MLE…(etc.). On phone, use phonetics for the letter or letters following the HX, to ensure accuracy. |
|  |  |
|  |  |
|  | ‡ new |
|  |  |
|  |  |
| HXA | Collect landline delivery authorize by addressee within \_\_\_\_ miles. (If no number, authorization is unlimited). |
|  |  |
| HXB | Cancel message if not delivered within \_\_\_\_ hours of filing time; service originating station. |
|  |  |
| HXC | Report date and time of delivery (TOD) to originating station. |
|  |  |
| HXD | Report to originating station the identity of station from which received, plus date and time. Report identity of station to which relayed, plus date and time, or if delivered report date, time and method of delivery. |
|  |  |
| HXE | Delivering station get reply from addressee, originate message back. |
|  |  |
| HXF | Hold delivery until \_\_\_\_\_ (date). |
|  |  |
| HXG | Delivery by mail or landline toll call not required. If toll or other expense involved, cancel message and service originating station. |
|  |  |
| HXI | Please handle as ICS-213. |
|  |  |
| HXR | Please confirm actual receipt by addressee, and notify the originator. |